    PAD Specification File
    ***************************

    PART TYPE:        LIFCL-17
    Performance Grade:      9_High-Performance_1.0V
    PACKAGE:          QFN72
    Package Status:                     Final          Version 23

    Wed Jun  5 12:16:59 2024

    Pinout by Port Name:
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | Port Name | Pin/Bank | Buffer Type  | Site  | Properties                                                                                                                                                          |
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | Clk       | 59/0     | LVCMOS33_IN  | PT59A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | En1       | 56/0     | LVCMOS33_IN  | PT61A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | out2[0]   | 52/0     | LVCMOS33_OUT | PT65A | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | out2[1]   | 53/0     | LVCMOS33_OUT | PT65B | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | out2[2]   | 55/0     | LVCMOS33_OUT | PT63B | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | out2[3]   | 43/1     | LVCMOS33_OUT | PR9B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | out2[4]   | 42/1     | LVCMOS33_OUT | PR7A  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | out2[5]   | 57/0     | LVCMOS33_OUT | PT61B | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | out2[6]   | 51/0     | LVCMOS33_OUT | PT63A | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | out2[7]   | 44/1     | LVCMOS33_OUT | PR7B  | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 0    | 3.3V  |
    | 1    | 3.3V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +----------------+-----------------------+------------+--------------+--------------+-----------------------------------------------------------+
    | Pin/Bank       | Pin Info              | Preference | Buffer Type  | Site         | Dual Function                                             |
    +----------------+-----------------------+------------+--------------+--------------+-----------------------------------------------------------+
    | 1/60           |                       |            |              | DPHY0_DP2    |                                                           |
    | 2/60           |                       |            |              | DPHY0_DN2    |                                                           |
    | 3/60           |                       |            |              | DPHY0_DN0    |                                                           |
    | 4/60           |                       |            |              | DPHY0_DP0    |                                                           |
    | 8/5            |     unused, PULL:DOWN |            |              | PB30B        | PCLKC5_3/CDR1_TESTN/VREF5_2/BDQ22                         |
    | 9/5            |     unused, PULL:DOWN |            |              | PB30A        | PCLKT5_3/CDR1_TESTP/BDQ22                                 |
    | 10/5           |     unused, PULL:DOWN |            |              | PB20B        | PCLKC5_1/LLC_GPLL0C_IN/ADC_CN3/BDQ22                      |
    | 11/5           |     unused, PULL:DOWN |            |              | PB20A        | PCLKT5_1/LLC_GPLL0T_IN/ADC_CP3/BDQ22                      |
    | 13/5           |     unused, PULL:DOWN |            |              | PB16B        | CDR_RXN0/ADC_CN0/COMP1N/BDQ22                             |
    | 14/5           |     unused, PULL:DOWN |            |              | PB16A        | LLC_GPLL0T_MFGOUT1/CDR_RXP0/VREF5_1/ADC_CP0/COMP1P/BDQ22  |
    | 15/5           |     unused, PULL:DOWN |            |              | PB18B        | PCLKC5_0/CDR_RXN1/ADC_CN1/COMP2N/BDQ22                    |
    | 16/5           |     unused, PULL:DOWN |            |              | PB18A        | PCLKT5_0/LLC_GPLL0T_MFGOUT2/CDR_RXP1/ADC_CP1/COMP2P/BDQ22 |
    | 19/5           |     unused, PULL:DOWN |            |              | PB26A        | PCLKT5_2/CDR0_TESTP/ADC_CP2/COMP3P/BDQ22                  |
    | 20/5           |     unused, PULL:DOWN |            |              | PB26B        | PCLKC5_2/CDR0_TESTN/ADC_CN2/COMP3N/BDQ22                  |
    | 22/3           |     unused, PULL:DOWN |            |              | PB56A        | PCLKT3_0/VREF3_1/ADC_CP5/BDQ62                            |
    | 23/3           |     unused, PULL:DOWN |            |              | PB56B        | PCLKC3_0/ADC_CN5/BDQ62                                    |
    | 24/3           |     unused, PULL:DOWN |            |              | PB60A        | PCLKT3_1/ADC_CP6/BDQ62                                    |
    | 25/3           |     unused, PULL:DOWN |            |              | PB60B        | PCLKC3_1/ADC_CN6/BDQ62                                    |
    | 27/3           |     unused, PULL:DOWN |            |              | PB64A        | ADC_CP8/BDQ62                                             |
    | 28/3           |     unused, PULL:DOWN |            |              | PB64B        | ADC_CN8/BDQ62                                             |
    | 30/3           |     unused, PULL:DOWN |            |              | PB66A        | PCLKT3_2/ADC_CP13/LRC_GPLL0T_MFGOUT1/BDQ62                |
    | 31/3           |     unused, PULL:DOWN |            |              | PB66B        | PCLKC3_2/ADC_CN13/LRC_GPLL0T_MFGOUT2/BDQ62                |
    | 33/3           |     unused, PULL:DOWN |            |              | PB68A        | PCLKT3_3/ADC_CP14/BDQ62                                   |
    | 34/3           |     unused, PULL:DOWN |            |              | PB68B        | PCLKC3_3/ADC_CN14/BDQ62                                   |
    | 36/3           |     unused, PULL:DOWN |            |              | PB70A        | LRC_GPLL0T_IN/ATB_FORCE/BDQ62                             |
    | 37/3           |     unused, PULL:DOWN |            |              | PB70B        | LRC_GPLL0C_IN/VREF3_2/ATB_SENSE/BDQ62                     |
    | 41/1           | Reserved: sysCONFIG   |            |              | PR9A         | TCK/SCLK/PMU_EXT_CLK/S9_IN                                |
    | 42/1           | out2[4]               |            | LVCMOS33_OUT | PR7A         | SD3/SDA/USER_SDA/S4_IN                                    |
    | 43/1           | out2[3]               |            | LVCMOS33_OUT | PR9B         | PMU_WAKEUPN/S4_OUT/EIO                                    |
    | 44/1           | out2[7]               |            | LVCMOS33_OUT | PR7B         | SD2/SCL/USER_SCL/S3_IN                                    |
    | 45/1           | Reserved: sysCONFIG   |            |              | PR5B         | TDO/SSO/SD1/S3_OUT                                        |
    | 46/1           | Reserved: sysCONFIG   |            |              | PR5A         | TDI/SSI/SD0/S5_OUT                                        |
    | 48/1           | Reserved: sysCONFIG   |            |              | PR3B         | TMS/SCSN/S5_IN                                            |
    | 51/0           | out2[6]               |            | LVCMOS33_OUT | PT63A        | MISO/MD1/SD5/S2_IN/OSC_HI                                 |
    | 52/0           | out2[0]               |            | LVCMOS33_OUT | PT65A        | MD3/SD7/S6_IN/OSC_BURST                                   |
    | 53/0           | out2[1]               |            | LVCMOS33_OUT | PT65B        | MCSNO/MSDO/S6_OUT                                         |
    | 55/0           | out2[2]               |            | LVCMOS33_OUT | PT63B        | MD2/SD6/S2_OUT                                            |
    | 56/0           | En1                   |            | LVCMOS33_IN  | PT61A        | MCSN/S1_IN/PCLKT0_1                                       |
    | 57/0           | out2[5]               |            | LVCMOS33_OUT | PT61B        | MOSI/MD0/SD4/S1_OUT                                       |
    | 58/0           | Reserved: sysCONFIG   |            |              | PT59B        | DONE/S0_OUT                                               |
    | 59/0           | Clk                   |            | LVCMOS33_IN  | PT59A        | MCLK/S0_IN/PCLKT0_0                                       |
    | 60/0           | Reserved: sysCONFIG   |            |              | PT57B        | PROGRAMN                                                  |
    | 61/0           | Reserved: sysCONFIG   |            |              | PT57A        | INITN                                                     |
    | 64/60          |                       |            |              | DPHY0_DP3    |                                                           |
    | 65/60          |                       |            |              | DPHY0_DN3    |                                                           |
    | 66/60          |                       |            |              | DPHY0_DP1    |                                                           |
    | 67/60          |                       |            |              | DPHY0_DN1    |                                                           |
    | 68/60          |                       |            |              | DPHY0_CKP    |                                                           |
    | 69/60          |                       |            |              | DPHY0_CKN    |                                                           |
    | ADC_DN0/70     |                       |            |              | ADC_DN0      |                                                           |
    | ADC_DN1/70     |                       |            |              | ADC_DN1      |                                                           |
    | ADC_DP0/70     |                       |            |              | ADC_DP0      |                                                           |
    | ADC_DP1/70     |                       |            |              | ADC_DP1      |                                                           |
    | APIO_R25C74E/0 |                       |            |              | APIO_R25C74E |                                                           |
    | DPHY1_CKN/61   |                       |            |              | DPHY1_CKN    |                                                           |
    | DPHY1_CKP/61   |                       |            |              | DPHY1_CKP    |                                                           |
    | DPHY1_DN0/61   |                       |            |              | DPHY1_DN0    |                                                           |
    | DPHY1_DN1/61   |                       |            |              | DPHY1_DN1    |                                                           |
    | DPHY1_DN2/61   |                       |            |              | DPHY1_DN2    |                                                           |
    | DPHY1_DN3/61   |                       |            |              | DPHY1_DN3    |                                                           |
    | DPHY1_DP0/61   |                       |            |              | DPHY1_DP0    |                                                           |
    | DPHY1_DP1/61   |                       |            |              | DPHY1_DP1    |                                                           |
    | DPHY1_DP2/61   |                       |            |              | DPHY1_DP2    |                                                           |
    | DPHY1_DP3/61   |                       |            |              | DPHY1_DP3    |                                                           |
    | PB22A/5        |     unused, PULL:DOWN |            |              | PB22A        | BDQS22                                                    |
    | PB22B/5        |     unused, PULL:DOWN |            |              | PB22B        | BDQSN22                                                   |
    | PB24A/5        |     unused, PULL:DOWN |            |              | PB24A        | BDQ22                                                     |
    | PB24B/5        |     unused, PULL:DOWN |            |              | PB24B        | BDQ22                                                     |
    | PB28A/5        |     unused, PULL:DOWN |            |              | PB28A        | BDQ22                                                     |
    | PB28B/5        |     unused, PULL:DOWN |            |              | PB28B        | BDQ22                                                     |
    | PB40A/4        |     unused, PULL:DOWN |            |              | PB40A        | VREF4_1/BDQ46                                             |
    | PB40B/4        |     unused, PULL:DOWN |            |              | PB40B        | BDQ46                                                     |
    | PB42A/4        |     unused, PULL:DOWN |            |              | PB42A        | PCLKT4_3/BDQ46                                            |
    | PB42B/4        |     unused, PULL:DOWN |            |              | PB42B        | PCLKC4_3/BDQ46                                            |
    | PB44A/4        |     unused, PULL:DOWN |            |              | PB44A        | BDQ46                                                     |
    | PB44B/4        |     unused, PULL:DOWN |            |              | PB44B        | BDQ46                                                     |
    | PB46A/4        |     unused, PULL:DOWN |            |              | PB46A        | BDQS46                                                    |
    | PB46B/4        |     unused, PULL:DOWN |            |              | PB46B        | BDQSN46                                                   |
    | PB48A/4        |     unused, PULL:DOWN |            |              | PB48A        | PCLKT4_2/BDQ46                                            |
    | PB48B/4        |     unused, PULL:DOWN |            |              | PB48B        | PCLKC4_2/BDQ46                                            |
    | PB50A/4        |     unused, PULL:DOWN |            |              | PB50A        | BDQ46                                                     |
    | PB50B/4        |     unused, PULL:DOWN |            |              | PB50B        | BDQ46                                                     |
    | PB52A/4        |     unused, PULL:DOWN |            |              | PB52A        | PCLKT4_1/BDQ46                                            |
    | PB52B/4        |     unused, PULL:DOWN |            |              | PB52B        | PCLKC4_1/BDQ46                                            |
    | PB54A/4        |     unused, PULL:DOWN |            |              | PB54A        | PCLKT4_0/BDQ46                                            |
    | PB54B/4        |     unused, PULL:DOWN |            |              | PB54B        | PCLKC4_0/VREF4_2/BDQ46                                    |
    | PB58A/3        |     unused, PULL:DOWN |            |              | PB58A        | ADC_CP7/BDQ62                                             |
    | PB58B/3        |     unused, PULL:DOWN |            |              | PB58B        | ADC_CN7/BDQ62                                             |
    | PB62A/3        |     unused, PULL:DOWN |            |              | PB62A        | ADC_CP9/BDQS62                                            |
    | PB62B/3        |     unused, PULL:DOWN |            |              | PB62B        | ADC_CN9/BDQSN62                                           |
    | PR11A/1        |     unused, PULL:DOWN |            |              | PR11A        | EIO                                                       |
    | PR11B/1        |     unused, PULL:DOWN |            |              | PR11B        | PCLKT1_2/EIO                                              |
    | PR13A/1        |     unused, PULL:DOWN |            |              | PR13A        | PCLKT1_1/EIO                                              |
    | PR13B/1        |     unused, PULL:DOWN |            |              | PR13B        | PCLKT1_0/EIO                                              |
    | PT67A/0        |     unused, PULL:DOWN |            |              | PT67A        | S7_IN                                                     |
    | PT67B/0        |     unused, PULL:DOWN |            |              | PT67B        | S7_OUT                                                    |
    +----------------+-----------------------+------------+--------------+--------------+-----------------------------------------------------------+

    sysCONFIG Pins:
    +----------+----------------------------+----------+-------------+
    | Pad Name | sysCONFIG Pin Name         | Pin/Bank | Buffer Type |
    +----------+----------------------------+----------+-------------+
    | PT57A    | INITN                      | 61/0     |             |
    | PT57B    | PROGRAMN                   | 60/0     |             |
    | PT59B    | DONE/S0_OUT                | 58/0     |             |
    | PR9A     | TCK/SCLK/PMU_EXT_CLK/S9_IN | 41/1     |             |
    | PR5A     | TDI/SSI/SD0/S5_OUT         | 46/1     |             |
    | PR5B     | TDO/SSO/SD1/S3_OUT         | 45/1     |             |
    | PR3B     | TMS/SCSN/S5_IN             | 48/1     |             |
    +----------+----------------------------+----------+-------------+

    Locate Constraints for each Pin:

    ldc_set_location -site {59} [ get_ports {Clk} ]
    ldc_set_location -site {56} [ get_ports {En1} ]
    ldc_set_location -site {52} [ get_ports {out2[0]} ]
    ldc_set_location -site {53} [ get_ports {out2[1]} ]
    ldc_set_location -site {55} [ get_ports {out2[2]} ]
    ldc_set_location -site {43} [ get_ports {out2[3]} ]
    ldc_set_location -site {42} [ get_ports {out2[4]} ]
    ldc_set_location -site {57} [ get_ports {out2[5]} ]
    ldc_set_location -site {51} [ get_ports {out2[6]} ]
    ldc_set_location -site {44} [ get_ports {out2[7]} ]

    Copyright (c) 2002-2022 Lattice Semiconductor Corporation,  All rights reserved.

    Wed Jun  5 12:16:59 2024