    PAD Specification File
    ***************************

    PART TYPE:        LFCPNX-50
    Performance Grade:      9_High-Performance_1.0V
    PACKAGE:          ASG256
    Package Status:                     Final          Version 16

    Thu Jun  6 10:01:55 2024

    Pinout by Port Name:
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | Port Name | Pin/Bank | Buffer Type  | Site  | Properties                                                                                                                                                          |
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+
    | A         | J6/2     | LVCMOS33_IN  | PR42B | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | B         | J2/2     | LVCMOS33_IN  | PR44B | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | ClkA      | J16/6    | LVCMOS33_IN  | PL42A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | ClkB      | J11/6    | LVCMOS33_IN  | PL44A | DRIVE:NA SLEWRATE:NA GLITCHFILTER:ON HYSTERESIS:ON TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:DOWN CLAMP:ON VREF:OFF     |
    | out1      | J7/2     | LVCMOS33_OUT | PR42A | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    | out2      | K2/2     | LVCMOS33_OUT | PR44A | DRIVE:8mA SLEWRATE:MED GLITCHFILTER:OFF HYSTERESIS:NA TERMINATION:OFF OPENDRAIN:OFF IO_TYPE:LVCMOS33 DIFFRESISTOR:OFF DIFFDRIVE:NA PULLMODE:NONE CLAMP:OFF VREF:OFF |
    +-----------+----------+--------------+-------+---------------------------------------------------------------------------------------------------------------------------------------------------------------------+

    Vccio by Bank:
    +------+-------+
    | Bank | Vccio |
    +------+-------+
    | 2    | 3.3V  |
    | 6    | 3.3V  |
    +------+-------+

    Vref by Bank:
    +------+-----+-----------------+---------+
    | Vref | Pin | Bank # / Vref # | Load(s) |
    +------+-----+-----------------+---------+
    +------+-----+-----------------+---------+

    Pinout by Pin Number:
    +-----------------+-----------------------+------------+--------------+-----------------+----------------------------------------------------------+
    | Pin/Bank        | Pin Info              | Preference | Buffer Type  | Site            | Dual Function                                            |
    +-----------------+-----------------------+------------+--------------+-----------------+----------------------------------------------------------+
    | A2/83           |                       |            |              | SD_EXT1_REFCLKP |                                                          |
    | A5/80           |                       |            |              | SD3_TXDN        |                                                          |
    | A6/80           |                       |            |              | SD3_TXDP        |                                                          |
    | A8/80           |                       |            |              | SD2_TXDN        |                                                          |
    | A9/80           |                       |            |              | SD2_TXDP        |                                                          |
    | A11/80          |                       |            |              | SD1_TXDN        |                                                          |
    | A12/80          |                       |            |              | SD1_TXDP        |                                                          |
    | A14/80          |                       |            |              | SD0_TXDN        |                                                          |
    | A15/80          |                       |            |              | SD0_TXDP        |                                                          |
    | B1/83           |                       |            |              | SD_EXT1_REFCLKN |                                                          |
    | B2/83           |                       |            |              | SD_EXT0_REFCLKP |                                                          |
    | B3/83           |                       |            |              | SD_EXT0_REFCLKN |                                                          |
    | B6/80           |                       |            |              | SD3_REXT        |                                                          |
    | B8/80           |                       |            |              | SD3_REFRET      |                                                          |
    | B10/80          |                       |            |              | SD1_RXDN        |                                                          |
    | B12/80          |                       |            |              | SD1_REFRET      |                                                          |
    | B13/80          |                       |            |              | SD1_REXT        |                                                          |
    | C1/0            |     unused, PULL:DOWN |            |              | PT144B          | S7_OUT                                                   |
    | C2/0            |     unused, PULL:DOWN |            |              | PT144A          | S7_IN                                                    |
    | C3/0            |     unused, PULL:DOWN |            |              | PT140B          | MD2/SD6/S2_OUT                                           |
    | C4/0            |     unused, PULL:DOWN |            |              | PT140A          | MISO/MD1/SD5/S2_IN/OSC_HI                                |
    | C5/80           |                       |            |              | SD3_RXDN        |                                                          |
    | C6/80           |                       |            |              | SD3_RXDP        |                                                          |
    | C8/80           |                       |            |              | SD2_RXDP        |                                                          |
    | C9/80           |                       |            |              | SD2_RXDN        |                                                          |
    | C11/80          |                       |            |              | SD1_RXDP        |                                                          |
    | C13/80          |                       |            |              | SD0_RXDP        |                                                          |
    | C14/80          |                       |            |              | SD0_RXDN        |                                                          |
    | C15/80          |                       |            |              | SD0_REFRET      |                                                          |
    | C16/80          |                       |            |              | SD0_REXT        |                                                          |
    | D1/0            |     unused, PULL:DOWN |            |              | PT142B          | MCSNO/MSDO/S6_OUT                                        |
    | D2/0            |     unused, PULL:DOWN |            |              | PT142A          | MD3/SD7/S6_IN/OSC_BURST                                  |
    | D3/0            |     unused, PULL:DOWN |            |              | PT138B          | MOSI/MD0/SD4/S1_OUT                                      |
    | D4/0            |     unused, PULL:DOWN |            |              | PT138A          | MCSN/S1_IN/PCLKT0_1                                      |
    | D5/0            | Reserved: sysCONFIG   |            |              | PT136B          | DONE/S0_OUT                                              |
    | D7/0            | Reserved: sysCONFIG   |            |              | PT134B          | PROGRAMN                                                 |
    | D8/80           |                       |            |              | SD2_REFRET      |                                                          |
    | D10/80          |                       |            |              | SDQ0_REFCLKN    |                                                          |
    | D15/7           |     unused, PULL:DOWN |            |              | PL3A            | ULC_GPLL0T_IN/EIO                                        |
    | D16/7           |     unused, PULL:DOWN |            |              | PL3B            | EIO                                                      |
    | E1/1            | Reserved: sysCONFIG   |            |              | PR13A           | TCK/SCLK/PMU_EXT_CLK                                     |
    | E2/1            |     unused, PULL:DOWN |            |              | PR11A           | SD3/SDA/USER_SDA/S4_IN                                   |
    | E3/1            |     unused, PULL:DOWN |            |              | PR10A           | EIO                                                      |
    | E5/0            |     unused, PULL:DOWN |            |              | PT136A          | MCLK/PCLKT0_0/S0_IN                                      |
    | E6/1            |     unused, PULL:DOWN |            |              | PR3B            | S8_IN/EIO                                                |
    | E7/0            | Reserved: sysCONFIG   |            |              | PT134A          | INITN                                                    |
    | E8/80           |                       |            |              | SD2_REXT        |                                                          |
    | E10/80          |                       |            |              | SDQ0_REFCLKP    |                                                          |
    | E12/7           |     unused, PULL:DOWN |            |              | PL4A            | ULC_GPLL0T_MFGOUT1/EIO                                   |
    | E13/7           |     unused, PULL:DOWN |            |              | PL4B            | ULC_GPLL0T_MFGOUT2/EIO                                   |
    | E14/7           |     unused, PULL:DOWN |            |              | PL6A            | EIO                                                      |
    | E15/7           |     unused, PULL:DOWN |            |              | PL6B            | EIO                                                      |
    | E16/7           |     unused, PULL:DOWN |            |              | PL11A           | EIO                                                      |
    | F1/1            |     unused, PULL:DOWN |            |              | PR13B           | PMU_WAKEUPN/SD11/S4_OUT                                  |
    | F2/1            |     unused, PULL:DOWN |            |              | PR11B           | SD2/SCL/USER_SCL/S3_IN                                   |
    | F3/1            | Reserved: sysCONFIG   |            |              | PR10B           | TDO/SSO/SD1/S3_OUT                                       |
    | F5/1            | Reserved: sysCONFIG   |            |              | PR8B            | TDI/SSI/SD0/S5_OUT                                       |
    | F6/1            |     unused, PULL:DOWN |            |              | PR8A            | EIO                                                      |
    | F7/1            |     unused, PULL:DOWN |            |              | PR6A            | URC_GPLL0T_MFGOUT1/EIO                                   |
    | F9/1            |     unused, PULL:DOWN |            |              | PR4B            | SD10                                                     |
    | F10/1           |     unused, PULL:DOWN |            |              | PR4A            | URC_GPLL0T_IN/S8_OUT/EIO                                 |
    | F11/7           |     unused, PULL:DOWN |            |              | PL8A            | EIO                                                      |
    | F12/7           |     unused, PULL:DOWN |            |              | PL8B            | EIO                                                      |
    | F14/7           |     unused, PULL:DOWN |            |              | PL10A           | EIO                                                      |
    | F15/7           |     unused, PULL:DOWN |            |              | PL10B           | EIO                                                      |
    | F16/7           |     unused, PULL:DOWN |            |              | PL11B           | EIO                                                      |
    | G1/1            |     unused, PULL:DOWN |            |              | PR31A           | PCLKT1_0/EIO                                             |
    | G2/1            |     unused, PULL:DOWN |            |              | PR17B           | SD13                                                     |
    | G3/1            |     unused, PULL:DOWN |            |              | PR17A           | SD12                                                     |
    | G5/1            |     unused, PULL:DOWN |            |              | PR15B           | SD8                                                      |
    | G6/1            |     unused, PULL:DOWN |            |              | PR15A           | SD9                                                      |
    | G7/1            | Reserved: sysCONFIG   |            |              | PR6B            | TMS/SCSN/URC_GPLL0T_MFGOUT2/S5_IN                        |
    | G9/7            |     unused, PULL:DOWN |            |              | PL13A           | EIO                                                      |
    | G10/7           |     unused, PULL:DOWN |            |              | PL13B           | EIO                                                      |
    | G11/7           |     unused, PULL:DOWN |            |              | PL15A           | EIO                                                      |
    | G12/7           |     unused, PULL:DOWN |            |              | PL15B           | EIO                                                      |
    | G14/7           |     unused, PULL:DOWN |            |              | PL17A           | EIO                                                      |
    | G15/7           |     unused, PULL:DOWN |            |              | PL17B           | EIO                                                      |
    | G16/7           |     unused, PULL:DOWN |            |              | PL19A           | EIO                                                      |
    | H1/1            |     unused, PULL:DOWN |            |              | PR31B           | EIO                                                      |
    | H2/1            |     unused, PULL:DOWN |            |              | PR29B           | EIO                                                      |
    | H3/1            |     unused, PULL:DOWN |            |              | PR29A           | PCLKT1_1/EIO                                             |
    | H4/1            |     unused, PULL:DOWN |            |              | PR28B           | EIO                                                      |
    | H5/1            |     unused, PULL:DOWN |            |              | PR28A           | PCLKT1_2/EIO                                             |
    | H6/1            |     unused, PULL:DOWN |            |              | PR19B           | SD15                                                     |
    | H7/1            |     unused, PULL:DOWN |            |              | PR19A           | SD14                                                     |
    | H9/7            |     unused, PULL:DOWN |            |              | PL28A           | PCLKT7_2/EIO                                             |
    | H10/7           |     unused, PULL:DOWN |            |              | PL28B           | EIO                                                      |
    | H11/7           |     unused, PULL:DOWN |            |              | PL29A           | PCLKT7_1/EIO                                             |
    | H12/7           |     unused, PULL:DOWN |            |              | PL29B           | EIO                                                      |
    | H14/7           |     unused, PULL:DOWN |            |              | PL31A           | PCLKT7_0/EIO                                             |
    | H15/7           |     unused, PULL:DOWN |            |              | PL31B           | EIO                                                      |
    | H16/7           |     unused, PULL:DOWN |            |              | PL19B           | EIO                                                      |
    | J1/2            |     unused, PULL:DOWN |            |              | PR46B           | EIO                                                      |
    | J2/2            | B                     |            | LVCMOS33_IN  | PR44B           | EIO                                                      |
    | J6/2            | A                     |            | LVCMOS33_IN  | PR42B           | EIO                                                      |
    | J7/2            | out1                  |            | LVCMOS33_OUT | PR42A           | PCLKT2_0/EIO                                             |
    | J8/6            |     unused, PULL:DOWN |            |              | PL46B           | EIO                                                      |
    | J9/6            |     unused, PULL:DOWN |            |              | PL46A           | PCLKT6_2/EIO                                             |
    | J10/6           |     unused, PULL:DOWN |            |              | PL44B           | EIO                                                      |
    | J11/6           | ClkB                  |            | LVCMOS33_IN  | PL44A           | PCLKT6_1/EIO                                             |
    | J12/5           |     unused, PULL:DOWN |            |              | PB38B           | BDQ42                                                    |
    | J15/6           |     unused, PULL:DOWN |            |              | PL42B           | EIO                                                      |
    | J16/6           | ClkA                  |            | LVCMOS33_IN  | PL42A           | PCLKT6_0/EIO                                             |
    | K1/2            |     unused, PULL:DOWN |            |              | PR46A           | PCLKT2_2/EIO                                             |
    | K2/2            | out2                  |            | LVCMOS33_OUT | PR44A           | PCLKT2_1/EIO                                             |
    | K3/3            |     unused, PULL:DOWN |            |              | PB156B          | LRC_GPLL0C_IN/VREF3_2/ATB_SENSE/BDQ150                   |
    | K4/3            |     unused, PULL:DOWN |            |              | PB146B          | ADC_CN14/BDQ150                                          |
    | K5/3            |     unused, PULL:DOWN |            |              | PB110B          | ADC_CN10/BDQ114                                          |
    | K6/3            |     unused, PULL:DOWN |            |              | PB110A          | VREF3_1/ADC_CP10/BDQ114                                  |
    | K7/4            |     unused, PULL:DOWN |            |              | PB100B          | PCLKC4_2/ADC_CN7/BDQ102                                  |
    | K8/4            |     unused, PULL:DOWN |            |              | PB100A          | PCLKT4_2/ADC_CP7/BDQ102                                  |
    | K9/4            |     unused, PULL:DOWN |            |              | PB58A           | PCLKT4_1/BDQ54                                           |
    | K10/4           |     unused, PULL:DOWN |            |              | PB50B           | BDQ54                                                    |
    | K11/4           |     unused, PULL:DOWN |            |              | PB50A           | VREF4_1/BDQ54                                            |
    | K12/5           |     unused, PULL:DOWN |            |              | PB38A           | BDQ42                                                    |
    | K13/5           |     unused, PULL:DOWN |            |              | PB34A           | BDQ30                                                    |
    | K14/5           |     unused, PULL:DOWN |            |              | PB26A           | BDQ30                                                    |
    | K15/5           |     unused, PULL:DOWN |            |              | PB10B           | PCLKC5_1/CDR0_TESTN/ADC_CN2/COMP3N/BDQ6                  |
    | K16/5           |     unused, PULL:DOWN |            |              | PB10A           | PCLKT5_1/CDR0_TESTP/ADC_CP2/COMP3P/BDQ6                  |
    | L1/70           |                       |            |              | ADC_DP0         |                                                          |
    | L3/3            |     unused, PULL:DOWN |            |              | PB156A          | LRC_GPLL0T_IN/ATB_FORCE/BDQ150                           |
    | L4/3            |     unused, PULL:DOWN |            |              | PB146A          | ADC_CP14/BDQ150                                          |
    | L5/3            |     unused, PULL:DOWN |            |              | PB118B          | PCLKC3_1/COMP2IN/BDQ114                                  |
    | L6/3            |     unused, PULL:DOWN |            |              | PB118A          | PCLKT3_1/COMP2IP/BDQ114                                  |
    | L7/4            |     unused, PULL:DOWN |            |              | PB98B           | ADC_CN5/BDQ102                                           |
    | L8/4            |     unused, PULL:DOWN |            |              | PB98A           | ADC_CP5/BDQ102                                           |
    | L9/4            |     unused, PULL:DOWN |            |              | PB58B           | PCLKC4_1/BDQ54                                           |
    | L10/4           |     unused, PULL:DOWN |            |              | PB56B           | BDQ54                                                    |
    | L11/5           |     unused, PULL:DOWN |            |              | PB46B           | PCLKC5_3/BDQ42                                           |
    | L12/5           |     unused, PULL:DOWN |            |              | PB46A           | PCLKT5_3/BDQ42                                           |
    | L13/5           |     unused, PULL:DOWN |            |              | PB34B           | BDQ30                                                    |
    | L14/5           |     unused, PULL:DOWN |            |              | PB26B           | BDQ30                                                    |
    | L15/5           |     unused, PULL:DOWN |            |              | PB6B            | BDQSN6                                                   |
    | L16/5           |     unused, PULL:DOWN |            |              | PB6A            | BDQS6                                                    |
    | M1/70           |                       |            |              | ADC_DN0         |                                                          |
    | M3/3            |     unused, PULL:DOWN |            |              | PB154B          | PCLKC3_3/LRC_GPLL0T_MFGOUT2/ADC_CN15/BDQ150              |
    | M4/3            |     unused, PULL:DOWN |            |              | PB116B          | ADC_CN8/BDQ114                                           |
    | M5/3            |     unused, PULL:DOWN |            |              | PB116A          | ADC_CP8/BDQ114                                           |
    | M6/4            |     unused, PULL:DOWN |            |              | PB106B          | PCLKC4_3/BDQ102                                          |
    | M7/4            |     unused, PULL:DOWN |            |              | PB106A          | PCLKT4_3/BDQ102                                          |
    | M10/4           |     unused, PULL:DOWN |            |              | PB56A           | BDQ54                                                    |
    | M11/5           |     unused, PULL:DOWN |            |              | PB48B           | VREF5_2/BDQ42                                            |
    | M12/5           |     unused, PULL:DOWN |            |              | PB48A           | BDQ42                                                    |
    | M13/5           |     unused, PULL:DOWN |            |              | PB28B           | BDQ30                                                    |
    | M14/5           |     unused, PULL:DOWN |            |              | PB28A           | BDQ30                                                    |
    | M15/5           |     unused, PULL:DOWN |            |              | PB2B            | LLC_GPLL0C_IN/CDR_RXN0/ADC_CN0/COMP1N/BDQ6               |
    | M16/5           |     unused, PULL:DOWN |            |              | PB2A            | LLC_GPLL0T_IN/CDR_RXP0/VREF5_1/ADC_CP0/COMP1P/BDQ6       |
    | N2/70           |                       |            |              | ADC_DP1         |                                                          |
    | N3/3            |     unused, PULL:DOWN |            |              | PB154A          | PCLKT3_3/LRC_GPLL0T_MFGOUT1/ADC_CP15/BDQ150              |
    | N4/3            |     unused, PULL:DOWN |            |              | PB120A          | ADC_CP13/BDQ114                                          |
    | N5/3            |     unused, PULL:DOWN |            |              | PB120B          | ADC_CN13/BDQ114                                          |
    | N6/4            |     unused, PULL:DOWN |            |              | PB108B          | VREF4_2/BDQ102                                           |
    | N7/4            |     unused, PULL:DOWN |            |              | PB108A          | BDQ102                                                   |
    | N15/5           |     unused, PULL:DOWN |            |              | PB4B            | PCLKC5_0/LLC_GPLL0T_MFGOUT2/CDR_RXN1/ADC_CN1/COMP2N/BDQ6 |
    | N16/5           |     unused, PULL:DOWN |            |              | PB4A            | PCLKT5_0/LLC_GPLL0T_MFGOUT1/CDR_RXP1/ADC_CP1/COMP2P/BDQ6 |
    | P2/70           |                       |            |              | ADC_DN1         |                                                          |
    | P9/4            |     unused, PULL:DOWN |            |              | PB60A           | BDQ54                                                    |
    | P10/4           |     unused, PULL:DOWN |            |              | PB60B           | BDQ54                                                    |
    | P11/5           |     unused, PULL:DOWN |            |              | PB40B           | PCLKC5_2/BDQ42                                           |
    | P12/5           |     unused, PULL:DOWN |            |              | PB40A           | PCLKT5_2/BDQ42                                           |
    | P13/5           |     unused, PULL:DOWN |            |              | PB32A           | BDQ30                                                    |
    | P14/5           |     unused, PULL:DOWN |            |              | PB32B           | BDQ30                                                    |
    | P15/5           |     unused, PULL:DOWN |            |              | PB8A            | ADC_CP3/BDQ6                                             |
    | P16/5           |     unused, PULL:DOWN |            |              | PB8B            | ADC_CN3/BDQ6                                             |
    | PB62A/4         |     unused, PULL:DOWN |            |              | PB62A           | BDQ66                                                    |
    | PB62B/4         |     unused, PULL:DOWN |            |              | PB62B           | BDQ66                                                    |
    | PB64A/4         |     unused, PULL:DOWN |            |              | PB64A           | BDQ66                                                    |
    | PB64B/4         |     unused, PULL:DOWN |            |              | PB64B           | BDQ66                                                    |
    | PB66A/4         |     unused, PULL:DOWN |            |              | PB66A           | BDQS66                                                   |
    | PB66B/4         |     unused, PULL:DOWN |            |              | PB66B           | BDQSN66                                                  |
    | PB80A/4         |     unused, PULL:DOWN |            |              | PB80A           | BDQ66                                                    |
    | PB80B/4         |     unused, PULL:DOWN |            |              | PB80B           | BDQ66                                                    |
    | PB82A/4         |     unused, PULL:DOWN |            |              | PB82A           | BDQ66                                                    |
    | PB82B/4         |     unused, PULL:DOWN |            |              | PB82B           | BDQ66                                                    |
    | PB84A/4         |     unused, PULL:DOWN |            |              | PB84A           | BDQ66                                                    |
    | PB84B/4         |     unused, PULL:DOWN |            |              | PB84B           | BDQ66                                                    |
    | PB86A/4         |     unused, PULL:DOWN |            |              | PB86A           | BDQ90                                                    |
    | PB86B/4         |     unused, PULL:DOWN |            |              | PB86B           | BDQ90                                                    |
    | PB88A/4         |     unused, PULL:DOWN |            |              | PB88A           | BDQ90                                                    |
    | PB88B/4         |     unused, PULL:DOWN |            |              | PB88B           | BDQ90                                                    |
    | PB90A/4         |     unused, PULL:DOWN |            |              | PB90A           | BDQS90                                                   |
    | PB90B/4         |     unused, PULL:DOWN |            |              | PB90B           | BDQSN90                                                  |
    | PB92A/4         |     unused, PULL:DOWN |            |              | PB92A           | BDQ90                                                    |
    | PB92B/4         |     unused, PULL:DOWN |            |              | PB92B           | BDQ90                                                    |
    | PB94A/4         |     unused, PULL:DOWN |            |              | PB94A           | BDQ90                                                    |
    | PB94B/4         |     unused, PULL:DOWN |            |              | PB94B           | BDQ90                                                    |
    | PB96A/4         |     unused, PULL:DOWN |            |              | PB96A           | BDQ90                                                    |
    | PB96B/4         |     unused, PULL:DOWN |            |              | PB96B           | BDQ90                                                    |
    | PB122A/3        |     unused, PULL:DOWN |            |              | PB122A          | BDQ126                                                   |
    | PB122B/3        |     unused, PULL:DOWN |            |              | PB122B          | BDQ126                                                   |
    | PB124A/3        |     unused, PULL:DOWN |            |              | PB124A          | BDQ126                                                   |
    | PB124B/3        |     unused, PULL:DOWN |            |              | PB124B          | BDQ126                                                   |
    | PB126A/3        |     unused, PULL:DOWN |            |              | PB126A          | BDQS126                                                  |
    | PB126B/3        |     unused, PULL:DOWN |            |              | PB126B          | BDQSN126                                                 |
    | PB128A/3        |     unused, PULL:DOWN |            |              | PB128A          | BDQ126                                                   |
    | PB128B/3        |     unused, PULL:DOWN |            |              | PB128B          | BDQ126                                                   |
    | PB130A/3        |     unused, PULL:DOWN |            |              | PB130A          | BDQ126                                                   |
    | PB130B/3        |     unused, PULL:DOWN |            |              | PB130B          | BDQ126                                                   |
    | PB132A/3        |     unused, PULL:DOWN |            |              | PB132A          | BDQ126                                                   |
    | PB132B/3        |     unused, PULL:DOWN |            |              | PB132B          | BDQ126                                                   |
    | PB134A/3        |     unused, PULL:DOWN |            |              | PB134A          | BDQ138                                                   |
    | PB134B/3        |     unused, PULL:DOWN |            |              | PB134B          | BDQ138                                                   |
    | PB136A/3        |     unused, PULL:DOWN |            |              | PB136A          | BDQ138                                                   |
    | PB136B/3        |     unused, PULL:DOWN |            |              | PB136B          | BDQ138                                                   |
    | PB138A/3        |     unused, PULL:DOWN |            |              | PB138A          | BDQS138                                                  |
    | PB138B/3        |     unused, PULL:DOWN |            |              | PB138B          | BDQSN138                                                 |
    | PB140A/3        |     unused, PULL:DOWN |            |              | PB140A          | BDQ138                                                   |
    | PB140B/3        |     unused, PULL:DOWN |            |              | PB140B          | BDQ138                                                   |
    | PB142A/3        |     unused, PULL:DOWN |            |              | PB142A          | BDQ138                                                   |
    | PB142B/3        |     unused, PULL:DOWN |            |              | PB142B          | BDQ138                                                   |
    | PB144A/3        |     unused, PULL:DOWN |            |              | PB144A          | BDQ138                                                   |
    | PB144B/3        |     unused, PULL:DOWN |            |              | PB144B          | BDQ138                                                   |
    | PL20A/7         |     unused, PULL:DOWN |            |              | PL20A           | EIO                                                      |
    | PL20B/7         |     unused, PULL:DOWN |            |              | PL20B           | EIO                                                      |
    | PL22A/7         |     unused, PULL:DOWN |            |              | PL22A           | EIO                                                      |
    | PL22B/7         |     unused, PULL:DOWN |            |              | PL22B           | EIO                                                      |
    | PL24A/7         |     unused, PULL:DOWN |            |              | PL24A           | EIO                                                      |
    | PL24B/7         |     unused, PULL:DOWN |            |              | PL24B           | EIO                                                      |
    | PL26A/7         |     unused, PULL:DOWN |            |              | PL26A           | EIO                                                      |
    | PL26B/7         |     unused, PULL:DOWN |            |              | PL26B           | EIO                                                      |
    | PL33A/7         |     unused, PULL:DOWN |            |              | PL33A           | EIO                                                      |
    | PL33B/7         |     unused, PULL:DOWN |            |              | PL33B           | EIO                                                      |
    | PL35A/7         |     unused, PULL:DOWN |            |              | PL35A           | EIO                                                      |
    | PL35B/7         |     unused, PULL:DOWN |            |              | PL35B           | EIO                                                      |
    | PL38A/7         |     unused, PULL:DOWN |            |              | PL38A           | EIO                                                      |
    | PL38B/7         |     unused, PULL:DOWN |            |              | PL38B           | EIO                                                      |
    | PL40A/6         |     unused, PULL:DOWN |            |              | PL40A           | EIO                                                      |
    | PL40B/6         |     unused, PULL:DOWN |            |              | PL40B           | EIO                                                      |
    | PL47A/6         |     unused, PULL:DOWN |            |              | PL47A           | EIO                                                      |
    | PL47B/6         |     unused, PULL:DOWN |            |              | PL47B           | EIO                                                      |
    | PL49A/6         |     unused, PULL:DOWN |            |              | PL49A           | EIO                                                      |
    | PL49B/6         |     unused, PULL:DOWN |            |              | PL49B           | EIO                                                      |
    | PL51A/6         |     unused, PULL:DOWN |            |              | PL51A           | EIO                                                      |
    | PL51B/6         |     unused, PULL:DOWN |            |              | PL51B           | EIO                                                      |
    | PL53A/6         |     unused, PULL:DOWN |            |              | PL53A           | EIO                                                      |
    | PL53B/6         |     unused, PULL:DOWN |            |              | PL53B           | EIO                                                      |
    | PL55A/6         |     unused, PULL:DOWN |            |              | PL55A           | EIO                                                      |
    | PL55B/6         |     unused, PULL:DOWN |            |              | PL55B           | EIO                                                      |
    | PL56A/6         |     unused, PULL:DOWN |            |              | PL56A           | EIO                                                      |
    | PL56B/6         |     unused, PULL:DOWN |            |              | PL56B           | EIO                                                      |
    | PL58A/6         |     unused, PULL:DOWN |            |              | PL58A           | EIO                                                      |
    | PL58B/6         |     unused, PULL:DOWN |            |              | PL58B           | EIO                                                      |
    | PL60A/6         |     unused, PULL:DOWN |            |              | PL60A           | EIO                                                      |
    | PL60B/6         |     unused, PULL:DOWN |            |              | PL60B           | EIO                                                      |
    | PL62A/6         |     unused, PULL:DOWN |            |              | PL62A           | EIO                                                      |
    | PL62B/6         |     unused, PULL:DOWN |            |              | PL62B           | EIO                                                      |
    | PL64A/6         |     unused, PULL:DOWN |            |              | PL64A           | EIO                                                      |
    | PL64B/6         |     unused, PULL:DOWN |            |              | PL64B           | EIO                                                      |
    | PL65A/6         |     unused, PULL:DOWN |            |              | PL65A           | EIO                                                      |
    | PL65B/6         |     unused, PULL:DOWN |            |              | PL65B           | EIO                                                      |
    | PL67A/6         |     unused, PULL:DOWN |            |              | PL67A           | EIO                                                      |
    | PL67B/6         |     unused, PULL:DOWN |            |              | PL67B           | EIO                                                      |
    | PR20A/1         |     unused, PULL:DOWN |            |              | PR20A           | EIO                                                      |
    | PR20B/1         |     unused, PULL:DOWN |            |              | PR20B           | EIO                                                      |
    | PR22A/1         |     unused, PULL:DOWN |            |              | PR22A           | EIO                                                      |
    | PR22B/1         |     unused, PULL:DOWN |            |              | PR22B           | EIO                                                      |
    | PR24A/1         |     unused, PULL:DOWN |            |              | PR24A           | EIO                                                      |
    | PR24B/1         |     unused, PULL:DOWN |            |              | PR24B           | EIO                                                      |
    | PR26A/1         |     unused, PULL:DOWN |            |              | PR26A           | EIO                                                      |
    | PR26B/1         |     unused, PULL:DOWN |            |              | PR26B           | EIO                                                      |
    | PR33A/1         |     unused, PULL:DOWN |            |              | PR33A           | EIO                                                      |
    | PR33B/1         |     unused, PULL:DOWN |            |              | PR33B           | EIO                                                      |
    | PR35A/1         |     unused, PULL:DOWN |            |              | PR35A           | EIO                                                      |
    | PR35B/1         |     unused, PULL:DOWN |            |              | PR35B           | EIO                                                      |
    | PR38A/1         |     unused, PULL:DOWN |            |              | PR38A           | EIO                                                      |
    | PR38B/1         |     unused, PULL:DOWN |            |              | PR38B           | EIO                                                      |
    | PR40A/2         |     unused, PULL:DOWN |            |              | PR40A           | EIO                                                      |
    | PR40B/2         |     unused, PULL:DOWN |            |              | PR40B           | EIO                                                      |
    | PR47A/2         |     unused, PULL:DOWN |            |              | PR47A           | EIO                                                      |
    | PR47B/2         |     unused, PULL:DOWN |            |              | PR47B           | EIO                                                      |
    | PR49A/2         |     unused, PULL:DOWN |            |              | PR49A           | EIO                                                      |
    | PR49B/2         |     unused, PULL:DOWN |            |              | PR49B           | EIO                                                      |
    | PR51A/2         |     unused, PULL:DOWN |            |              | PR51A           | EIO                                                      |
    | PR51B/2         |     unused, PULL:DOWN |            |              | PR51B           | EIO                                                      |
    | PR53A/2         |     unused, PULL:DOWN |            |              | PR53A           | EIO                                                      |
    | PR53B/2         |     unused, PULL:DOWN |            |              | PR53B           | EIO                                                      |
    | PR55A/2         |     unused, PULL:DOWN |            |              | PR55A           | EIO                                                      |
    | PR55B/2         |     unused, PULL:DOWN |            |              | PR55B           | EIO                                                      |
    | PR56A/2         |     unused, PULL:DOWN |            |              | PR56A           | EIO                                                      |
    | PR56B/2         |     unused, PULL:DOWN |            |              | PR56B           | EIO                                                      |
    | PR58A/2         |     unused, PULL:DOWN |            |              | PR58A           | EIO                                                      |
    | PR58B/2         |     unused, PULL:DOWN |            |              | PR58B           | EIO                                                      |
    | PR60A/2         |     unused, PULL:DOWN |            |              | PR60A           | EIO                                                      |
    | PR60B/2         |     unused, PULL:DOWN |            |              | PR60B           | EIO                                                      |
    | PR62A/2         |     unused, PULL:DOWN |            |              | PR62A           | EIO                                                      |
    | PR62B/2         |     unused, PULL:DOWN |            |              | PR62B           | EIO                                                      |
    | PR64A/2         |     unused, PULL:DOWN |            |              | PR64A           | EIO                                                      |
    | PR64B/2         |     unused, PULL:DOWN |            |              | PR64B           | EIO                                                      |
    | PR65A/2         |     unused, PULL:DOWN |            |              | PR65A           | EIO                                                      |
    | PR65B/2         |     unused, PULL:DOWN |            |              | PR65B           | EIO                                                      |
    | PR67A/2         |     unused, PULL:DOWN |            |              | PR67A           | EIO                                                      |
    | PR67B/2         |     unused, PULL:DOWN |            |              | PR67B           | EIO                                                      |
    | PT146A/0        |     unused, PULL:DOWN |            |              | PT146A          |                                                          |
    | PT146B/0        |     unused, PULL:DOWN |            |              | PT146B          |                                                          |
    | PT148A/0        |     unused, PULL:DOWN |            |              | PT148A          |                                                          |
    | PT148B/0        |     unused, PULL:DOWN |            |              | PT148B          |                                                          |
    | PT150A/0        |     unused, PULL:DOWN |            |              | PT150A          |                                                          |
    | PT150B/0        |     unused, PULL:DOWN |            |              | PT150B          |                                                          |
    | PT152A/0        |     unused, PULL:DOWN |            |              | PT152A          |                                                          |
    | PT152B/0        |     unused, PULL:DOWN |            |              | PT152B          |                                                          |
    | PT154A/0        |     unused, PULL:DOWN |            |              | PT154A          |                                                          |
    | PT154B/0        |     unused, PULL:DOWN |            |              | PT154B          |                                                          |
    | PT156A/0        |     unused, PULL:DOWN |            |              | PT156A          |                                                          |
    | PT156B/0        |     unused, PULL:DOWN |            |              | PT156B          |                                                          |
    | R1/3            |     unused, PULL:DOWN |            |              | PB152B          | ADC_CN12/BDQ150                                          |
    | R2/3            |     unused, PULL:DOWN |            |              | PB152A          | ADC_CP12/BDQ150                                          |
    | R3/3            |     unused, PULL:DOWN |            |              | PB150A          | ADC_CP11/BDQS150                                         |
    | R4/3            |     unused, PULL:DOWN |            |              | PB148B          | PCLKC3_2/COMP3IN/BDQ150                                  |
    | R5/3            |     unused, PULL:DOWN |            |              | PB114A          | COMP1IP/BDQS114                                          |
    | R6/3            |     unused, PULL:DOWN |            |              | PB112A          | PCLKT3_0/ADC_CP4/BDQ114                                  |
    | R7/4            |     unused, PULL:DOWN |            |              | PB104B          | ADC_CN9/BDQ102                                           |
    | R8/4            |     unused, PULL:DOWN |            |              | PB102A          | ADC_CP6/BDQS102                                          |
    | R9/4            |     unused, PULL:DOWN |            |              | PB52B           | PCLKC4_0/BDQ54                                           |
    | R10/4           |     unused, PULL:DOWN |            |              | PB54B           | BDQSN54                                                  |
    | R11/5           |     unused, PULL:DOWN |            |              | PB44B           | BDQ42                                                    |
    | R12/5           |     unused, PULL:DOWN |            |              | PB42B           | BDQSN42                                                  |
    | R13/5           |     unused, PULL:DOWN |            |              | PB36B           | BDQ30                                                    |
    | R14/5           |     unused, PULL:DOWN |            |              | PB30A           | BDQS30                                                   |
    | R15/5           |     unused, PULL:DOWN |            |              | PB12B           | CDR1_TESTN/BDQ6                                          |
    | R16/5           |     unused, PULL:DOWN |            |              | PB12A           | CDR1_TESTP/BDQ6                                          |
    | SD4_REFRET/81   |                       |            |              | SD4_REFRET      |                                                          |
    | SD4_REXT/81     |                       |            |              | SD4_REXT        |                                                          |
    | SD4_RXDN/81     |                       |            |              | SD4_RXDN        |                                                          |
    | SD4_RXDP/81     |                       |            |              | SD4_RXDP        |                                                          |
    | SD4_TXDN/81     |                       |            |              | SD4_TXDN        |                                                          |
    | SD4_TXDP/81     |                       |            |              | SD4_TXDP        |                                                          |
    | SD5_REFRET/81   |                       |            |              | SD5_REFRET      |                                                          |
    | SD5_REXT/81     |                       |            |              | SD5_REXT        |                                                          |
    | SD5_RXDN/81     |                       |            |              | SD5_RXDN        |                                                          |
    | SD5_RXDP/81     |                       |            |              | SD5_RXDP        |                                                          |
    | SD5_TXDN/81     |                       |            |              | SD5_TXDN        |                                                          |
    | SD5_TXDP/81     |                       |            |              | SD5_TXDP        |                                                          |
    | SD6_REFRET/81   |                       |            |              | SD6_REFRET      |                                                          |
    | SD6_REXT/81     |                       |            |              | SD6_REXT        |                                                          |
    | SD6_RXDN/81     |                       |            |              | SD6_RXDN        |                                                          |
    | SD6_RXDP/81     |                       |            |              | SD6_RXDP        |                                                          |
    | SD6_TXDN/81     |                       |            |              | SD6_TXDN        |                                                          |
    | SD6_TXDP/81     |                       |            |              | SD6_TXDP        |                                                          |
    | SD7_REFRET/81   |                       |            |              | SD7_REFRET      |                                                          |
    | SD7_REXT/81     |                       |            |              | SD7_REXT        |                                                          |
    | SD7_RXDN/81     |                       |            |              | SD7_RXDN        |                                                          |
    | SD7_RXDP/81     |                       |            |              | SD7_RXDP        |                                                          |
    | SD7_TXDN/81     |                       |            |              | SD7_TXDN        |                                                          |
    | SD7_TXDP/81     |                       |            |              | SD7_TXDP        |                                                          |
    | SDQ1_REFCLKN/81 |                       |            |              | SDQ1_REFCLKN    |                                                          |
    | SDQ1_REFCLKP/81 |                       |            |              | SDQ1_REFCLKP    |                                                          |
    | T3/3            |     unused, PULL:DOWN |            |              | PB150B          | ADC_CN11/BDQSN150                                        |
    | T4/3            |     unused, PULL:DOWN |            |              | PB148A          | PCLKT3_2/COMP3IP/BDQ150                                  |
    | T5/3            |     unused, PULL:DOWN |            |              | PB114B          | COMP1IN/BDQSN114                                         |
    | T6/3            |     unused, PULL:DOWN |            |              | PB112B          | PCLKC3_0/ADC_CN4/BDQ114                                  |
    | T7/4            |     unused, PULL:DOWN |            |              | PB104A          | ADC_CP9/BDQ102                                           |
    | T8/4            |     unused, PULL:DOWN |            |              | PB102B          | ADC_CN6/BDQSN102                                         |
    | T9/4            |     unused, PULL:DOWN |            |              | PB52A           | PCLKT4_0/BDQ54                                           |
    | T10/4           |     unused, PULL:DOWN |            |              | PB54A           | BDQS54                                                   |
    | T11/5           |     unused, PULL:DOWN |            |              | PB44A           | BDQ42                                                    |
    | T12/5           |     unused, PULL:DOWN |            |              | PB42A           | BDQS42                                                   |
    | T13/5           |     unused, PULL:DOWN |            |              | PB36A           | BDQ30                                                    |
    | T14/5           |     unused, PULL:DOWN |            |              | PB30B           | BDQSN30                                                  |
    +-----------------+-----------------------+------------+--------------+-----------------+----------------------------------------------------------+

    sysCONFIG Pins:
    +----------+-----------------------------------+----------+-------------+
    | Pad Name | sysCONFIG Pin Name                | Pin/Bank | Buffer Type |
    +----------+-----------------------------------+----------+-------------+
    | PT134A   | INITN                             | E7/0     |             |
    | PT134B   | PROGRAMN                          | D7/0     |             |
    | PT136B   | DONE/S0_OUT                       | D5/0     |             |
    | PR13A    | TCK/SCLK/PMU_EXT_CLK              | E1/1     |             |
    | PR10B    | TDO/SSO/SD1/S3_OUT                | F3/1     |             |
    | PR8B     | TDI/SSI/SD0/S5_OUT                | F5/1     |             |
    | PR6B     | TMS/SCSN/URC_GPLL0T_MFGOUT2/S5_IN | G7/1     |             |
    +----------+-----------------------------------+----------+-------------+

    Locate Constraints for each Pin:

    ldc_set_location -site {J6} [ get_ports {A} ]
    ldc_set_location -site {J2} [ get_ports {B} ]
    ldc_set_location -site {J16} [ get_ports {ClkA} ]
    ldc_set_location -site {J11} [ get_ports {ClkB} ]
    ldc_set_location -site {J7} [ get_ports {out1} ]
    ldc_set_location -site {K2} [ get_ports {out2} ]

    Copyright (c) 2002-2022 Lattice Semiconductor Corporation,  All rights reserved.

    Thu Jun  6 10:01:55 2024