                             Lattice Mapping Report File

    Design:  top
    Family:  LFCPNX
    Device:  LFCPNX-50
    Package: ASG256
    Performance Grade:  9_High-Performance_1.0V

    Mapper:    version Radiant Software (64-bit) 2023.2.1.288.0
    Mapped on: Thu Jun  6 10:01:32 2024

    Design Information

    Command line:   map -i lab07_impl_1_syn.udb -pdc C:/Users/ssyahril/Downloads/FAE
         _F2F_Training_Labs_V2/FAE_F2F_Training_Labs_V2/LAB_07/My.pdc -o
         lab07_impl_1_map.udb -mp lab07_impl_1.mrp -hierrpt -gui -msgset C:/Users/ss
         yahril/Downloads/FAE_F2F_Training_Labs_V2/FAE_F2F_Training_Labs_V2/LAB_07/p
         romote.xml

    Design Summary

       Number of registers:           8 out of 43477 (<1%)
          Number of SLICE         registers:    8 out of 43000 (<1%)
          Number of PIO Input     registers:    0 out of   159 (0%)
          Number of PIO Output    registers:    0 out of   159 (0%)
          Number of PIO Tri-State registers:    0 out of   159 (0%)
       Number of LUT4s:               2 out of 43000 (<1%)
          Number used as logic LUT4s:                          2
          Number used as distributed RAM:                      0 (6 per 16X4 RAM)
          Number used as ripple logic:                         0 (2 per CCU2)
       Number of PIOs used/reserved:   13 out of   159 (8%)
          Number of PIOs reserved:      7 (per sysConfig and/or prohibit constraint)
          Number of PIOs used:          6
            Number of PIOs used for single ended IO:         6
            Number of PIO pairs used for differential IO:    0
            Number allocated to regular speed PIOs:     6 out of   75 (8%)
            Number allocated to high speed PIOs:        0 out of   84 (0%)
       Number of Dedicated IO used for ADC/PCS/PCIE:    0 out of   34 (0%)
       Number of IDDR/ODDR/TDDR functions used:      0 out of   402 (0%)
       Number of IOs using at least one DDR function: 0 (0 differential)
       Number of Block RAMs:          0 out of 96 (0%)
       Number of Large RAMs:          0 out of 4 (0%)
       Number of Logical DSP Functions:
          Number of Pre-Adders (9+9):    0 out of 264 (0%)
          Number of Multipliers (18x18): 0 out of 132 (0%)
             Number of 9X9:        0 (1 18x18 = 2   9x9)
             Number of 18x18:      0 (1 18x18 = 1 18x18)
             Number of 18x36:      0 (2 18x18 = 1 18x36)
             Number of 36x36:      0 (4 18x18 = 1 36x36)
          Number of 54-bit Accumulators: 0 out of 66 (0%)
          Number of 18-bit Registers:    0 out of 264 (0%)
       Number of Physical DSP Components:
          Number of PREADD9:             0 out of 264 (0%)
          Number of MULT9:               0 out of 264 (0%)
          Number of MULT18:              0 out of 132 (0%)
          Number of MULT18X36:           0 out of 66 (0%)
          Number of MULT36:              0 out of 33 (0%)
          Number of ACC54:               0 out of 66 (0%)
          Number of REG18:               0 out of 264 (0%)
       Number of ALUREGs:             0 out of 1 (0%)
       Number of PLLs:                0 out of 3 (0%)
       Number of DDRDLLs:             0 out of 2 (0%)
       Number of DLLDELs:             0 out of 10 (0%)
       Number of DQSs:                0 out of 11 (0%)
       Number of DCSs:                0 out of 2 (0%)
       Number of DCCs:                0 out of 62 (0%)
       Number of PCLKDIVs:            0 out of 2 (0%)
       Number of ECLKDIVs:            0 out of 12 (0%)
       Number of ECLKSYNCs:           0 out of 12 (0%)
       Number of ADC Blocks:          0 out of 1 (0%)
       Number of SGMIICDRs:           0 out of 2 (0%)
       Number of PMUs:                0 out of 1 (0%)
       Number of BNKREF18s:           0 out of 3 (0%)
       Number of BNKREF33s:           0 out of 5 (0%)
       Number of I2CFIFOs:            0 out of 1 (0%)
       Number of Oscillators:         0 out of 1 (0%)
       Number of GSR:                 0 out of 1 (0%)
       Number of Cryptographic Block: 0 out of 1 (0%)
       Number of Config IP:           0 out of 1 (0%)
                     TSALL:           0 out of 1 (0%)
       Number of JTAG:                0 out of 1 (0%)
       Number of Config LMMI:         0 out of 1 (0%)
       Number of Config MULTIBOOT:    0 out of 1 (0%)
       Number of SED:                 0 out of 1 (0%)
       Number of Config WDT:          0 out of 1 (0%)
       Number of PCSs:                0 out of 1 (0%)
       Number of PCIE Link Layers:    0 out of 1 (0%)
       Number of Clocks:  2
          Net ClkA_c: 4 loads, 4 rising, 0 falling (Driver: Port ClkA)
          Net ClkB_c: 4 loads, 4 rising, 0 falling (Driver: Port ClkB)
       Number of Clock Enables:  0
       Number of LSRs:  0
       Top 10 highest fanout non-clock nets:
          Net A_Sig: 2 loads
          Net B_sig: 2 loads
          Net A_c: 1 loads
          Net A_Sig1: 1 loads
          Net B_sig1: 1 loads
          Net MyCDC01.A_Sig_adj_3: 1 loads
          Net MyCDC02.A_Sig: 1 loads
          Net out1_c_N_1: 1 loads
          Net out2_c: 1 loads
          Net out2_c_N_2: 1 loads

       Number of warnings:  0
       Number of errors:    0

    Design Errors/Warnings

       No errors or warnings present.

    IO (PIO) Attributes

    +---------------------+-----------+-----------+-------+-------+-----------+
    | IO Name             | Direction | Levelmode |  IO   |  IO   | Special   |
    |                     |           |  IO_TYPE  |  REG  |  DDR  | IO Buffer |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | out2                | OUTPUT    |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | A                   | INPUT     |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | out1                | OUTPUT    |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | ClkB                | INPUT     |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | ClkA                | INPUT     |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+
    | B                   | INPUT     |           |       |       |           |
    +---------------------+-----------+-----------+-------+-------+-----------+

    Removed logic

    Block GSR_INST undriven or does not drive anything - clipped.
    Block i33 was optimized away.
    Block i1 was optimized away.
    Block i33 was optimized away.

    ASIC Components

    Constraint Summary

       Total number of constraints: 7
       Total number of constraints dropped: 0

    Run Time and Memory Usage

       Total CPU Time: 6 secs
       Total REAL Time: 6 secs
       Peak Memory Usage: 637 MB
    Checksum -- map: c5a258b55a5e02cbdfa07e2dd3a84f134b4731c1
    Copyright (c) 1991-1994 by NeoCAD Inc. All rights reserved.
    Copyright (c) 1995
         AT&T Corp.   All rights reserved.
    Copyright (c) 1995-2001 Lucent
         Technologies Inc.  All rights reserved.
    Copyright (c) 2001 Agere Systems
         All rights reserved.
    Copyright (c) 2002-2023 Lattice Semiconductor
         Corporation,  All rights reserved.